**The technical specifications &Technical Offer (Annex II+III)**

***PART B. ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER**

**Contract title: PROC/1447/25/Framework Contract for the Supply of Tyres No. 15**

**Publication reference: PROC/1447/25**

**Columns 1-2 should be completed by the Contracting Authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the Contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the Contracting Authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words “compliant” or “yes” are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications..

**GENERAL MANDATORY REQUIREMENTS for TYRES**

The subject of the tender procedure is assortment of **high-quality** vehicle tires to be used on different makes and models of vehicles in all weather conditions, typical of the European climate zone/all season**,** and operated on hard and dirt roads. The tires offered should strictly adhere to the following general requirements.

* 1. **CERTIFICATES**- Certificate of compliance in accordance with ETRTO, ECE, DOT standards issued by any of the recognized European Scientific Centre, (in accordance with EC Directive: 92/23/EC-EC30, EC54, R117, EU Tyre Labelling Regulation 1222/2009) or equivalent certification. Minimum requirements as indicated in the below technical specifications- /documented/.
  2. **WARRANTY**-
* Warranty for minimum period of two years/ hidden faults.
* Tread life warranty minimum **45,000km.**
  1. **DATE OF PRODUCTION** - no later than **6 months** before the date of the delivery

**PLEASE NOTE THAT “RECONDITIONED TYRES” WILL NOT BE ACCEPTED.**

ETRTO – The European Tire and Rim Technical Organisation, Brussels

DOT – Department of Transportation (USA)

ECE – Economic Commission for Europe

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **1.** | * Tire dimension: 12.00 R 20 * To be suitable for: Mercedes 2631, Volvo NL10, Volvo FL10. * Load index minimum: 154 / 150 * Speed index minimum: K * Tubeless * Tread: Steering Axle * Other: Good Traction in all weather conditions.   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **2.** | * Tire dimension: 12.00 R 20 * To be suitable for: Mercedes 2631, Volvo NL10, Volvo FL10. * Load index minimum: 154 / 150 * Speed index minimum: K * Tubeless * Tread: Drive Axle * Other: Good Traction in all weather conditions. To be used in combination with the above.   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **3.** | * Tire dimension: 11 R 22.5 * To be suitable for; Iveco ML135 * Load index minimum: 148 / 145 * Speed index minimum: K * Tubeless * Tread: Steering Axle * Other: Good Traction in all weather conditions   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **4.** | * Tire dimension: 11 R 22.5 * To be suitable for; Iveco ML135 * Load index minimum: 148 / 145 * Speed index minimum: K * Tubeless * Tread: Drive Axle * Other: Good Traction in all weather conditions. To be used in combination with the above.   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **5.** | * Tire dimension: 12 R 22.5 * To be suitable for; Hyundai HD260 * Load index minimum: 152 / 148 * Speed index minimum: K * Tubeless * Tread: Steering Axle * Other: Good Traction in all weather conditions   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **6.** | * Tire dimension: 12 R 22.5 * To be suitable for; Hyundai HD260 * Load index minimum: 152 / 148 * Speed index minimum: K * Tubeless * Tread: Drive Axle * Other: Good Traction in all weather conditions. To be used in combination with the above.   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **7.** | Tire dimension: 315/80 R 22.5  To be suitable for; Volvo FL10  Load index minimum: 156 / 150  Speed index minimum: K  Tubeless  Tread: Steering Axle  Other: Good Traction in all weather conditions  **Estimated quantity required: 4** | |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **8.** | Tire dimension: 315/80 R 22.5  To be suitable for; Volvo FL10  Load index minimum: 156 / 150  Speed index minimum: K  Tubeless  Tread: Drive Axle  Other: Good Traction in all weather conditions. To be used in combination with item no 7.  **Estimated quantity required: 4** | |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **9.** | • | Tire dimension: 12 - 18 or 12.00 R 18 |  |  |  |
|  | • | To be suitable for: Torpedo T1 - Armored |  |  |  |
|  |  | Personnel Carrier |  |  |  |
|  | • | Load index minimum: 128 |  |  |  |
|  | • | Alternative load marking- E/10PR (10ply) will be accepted. |  |  |  |
|  | • | Load capacity of 1800kg and higher. |  |  |  |
|  | • | Speed index minimum: F |  |  |  |
|  | • | Tread: All Axles |  |  |  |
|  | • | Other: Good Traction in all weather conditions, good off-road capacities, multi- |  |  |  |
|  |  | purpose. |  |  |  |
|  |  | **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **10.** | * Tire dimension: 14.5 - 20 * To be suitable for: Torpedo T1 - Armored Personnel Carrier * Load index minimum: 136 * Speed index minimum: G * Tubeless * Tread: All Axles * Other: Good Traction in all weather conditions, good off-road capacities, multi-purpose. See thread type sample below.   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **11.** | * Tire dimension: 335/80 R 20 |  |  |  |
|  | * To be suitable for: Nyala RG31 - Armored |  |  |  |
|  | Personnel Carrier |  |  |  |
|  | * Load index minimum: 141 |  |  |  |
|  | * Speed index minimum: k |  |  |  |
|  | * Tubeless |  |  |  |
|  | * Tread: All Axles |  |  |  |
|  |  |  |  |  |
|  | * Other: Good Traction in all weather conditions, good off-road capacities, multi- |  |  |  |
|  | purpose. See thread type sample below. |  |  |  |
|  | **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **12.** | * Tire dimension: 395/85 R 20 |  |  |  |
|  | * To be suitable for: RILA - Armored |  |  |  |
|  | Personnel Carrier |  |  |  |
|  | * Load index minimum: 168 |  |  |  |
|  | * Speed index minimum: K |  |  |  |
|  | * Tubeless |  |  |  |
|  | * Tread: All Axles |  |  |  |
|  |  |  |  |  |
|  | * Other: Good Traction in all weather conditions, good off-road capacities, multi- |  |  |  |
|  | purpose. See thread type sample below. |  |  |  |
|  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **13.** | * Tire dimension: 12.00 R 24 or 325/95R24 * To be suitable for: Mercedes ACTROS 4850 8 x 8 * Load index minimum: 160 / 156 * Speed index minimum: K * Tubeless * Tread: Steering Axle * Other: Good Traction in all weather conditions. See Thread type sample below.   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **14.** | * Tire dimension: 12.00 R 24 or 325/95R24 |  |  |  |
|  | * To be suitable for: Mercedes ACTROS |  |  |  |
|  | 4850 8 x 8 |  |  |  |
|  | * Load index minimum: 160 / 156 |  |  |  |
|  | * Speed index minimum: K |  |  |  |
|  | * Tubeless |  |  |  |
|  | * Tread: Drive Axle |  |  |  |
|  |  |  |  |  |
|  | * Other: Good Traction in all weather conditions. See Thread type sample below. |  |  |  |
|  |  |  |  |  |
|  | **Estimated quantity required : 2** |  |  |  |
|  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **15.** | * Tire dimension: 8.25 R 16C * To be suitable for: Hyundai HD 120 * Load index minimum: 121 / 120 * Speed index minimum: L * Tubeless * Tread: All Axles * Other: Good Traction in all weather conditions   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **16.** | • | Tire dimension: 285/70 R 19.5 |  |  |  |
|  | • | To be suitable for: King – Low-bed trailer. |  |  |  |
|  | • | Load index minimum: 150 / 148 |  |  |  |
|  | • | Speed index minimum: J |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Trailer |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Good resistance against damage on sidewalls. |  |  |  |
|  |  | **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **17.** | * Tire dimension: 235/75 R 17.5 * To be suitable for: Metaco – Container-trailer. * Load index minimum: 143 / 141 * Speed index minimum: J * Tubeless * Tread: Trailer * Other: Good resistance against damage on sidewalls.   **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **18.** | * Tire dimension: 12:00 R 20 * To be suitable for: Fantuzzi FDC150-1200 Forklift 17ton * Load index minimum: 176 * Speed index minimum: A5 * Tread: Forklift - Industrial * Other: Special tire for forklift. See Thread type sample below     **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **19.** | * Tire dimension: 8.25 - 15 * To be suitable for: Daewoo D70S-2 Forklift 7ton * Load index minimum: 153 * Speed index minimum: A5 * Tread: Forklift - Industrial * Other: Special tire for forklift. See Thread type sample below     **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **20.** | * Tire dimension: 8.15 – 15 (alternative: 28 x 9 -15) * To be suitable for: Daewoo D30S-3 Forklift 3ton (front wheels) * Load index minimum: 146 * Speed index minimum: A5 * Tread: Forklift - Industrial * Other: Special tire for forklift. **Estimated quantity required: 2** |  |  |  |
| **21.** | * Tire dimension: 6.50 – 10 * To be suitable for: Daewoo D30S-3 Forklift 3ton (rear wheels) * Load index minimum: 128 * Speed index minimum: A5 * Tread: Forklift - Industrial * Other: Special tire for forklift. **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **22.** | • | Tire dimension: 12 - 16.5 |  |  |  |
|  | • | To be suitable for: Daewoo 1760XL Skid steer, Front-end loader |  |  |  |
|  | • | Load index minimum: 136 (140) |  |  |  |
|  | • | Speed index minimum: A4 (A3) |  |  |  |
|  | • | Tread: Skid steer – Industrial |  |  |  |
|  |  | • Other: Special tire for skid steer drive. |  |  |  |
|  |  |  |  |  |  |
|  |  | **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **23.** | * Tire dimension: 440/80 R 28 (alternative 16.9 – 28) * To be suitable for: JCB 4CX Backhoe Loader * Load index minimum: 156 * Speed index minimum: A8 * Tread: All Axles, mud grip * Other: Good Traction suitable for construction sites.   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **24.** | • | Tire dimension: 400/80 -24 (alternative |  |  |  |
|  |  | 15.5/80 – 24) |  |  |  |
|  | • | To be suitable for: Manitou 1440 |  |  |  |
|  |  | Teleporter – Telescopic Forklift |  |  |  |
|  | • | Load index minimum: 162 |  |  |  |
|  | • | Speed index minimum: A8 |  |  |  |
|  | • | Tread: All Axles, mud grip |  |  |  |
|  | • Other: Good Traction suitable for construction sites. | |  |  |  |
|  |  |  |  |  |  |
|  |  | **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **25.** | * Tire dimension: 14.9 – 24 * To be suitable for: Manitou 732 Teleporter – Telescopic Forklift * Load index minimum: 128 * Speed index minimum: A8 * Tread: All Axles, mud grip * Other: Good Traction suitable for construction sites.   **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **26.** | * Tire dimension: 195R14C * To be suitable for: Leyland-Daf -/Truck-Specialized (Cherry Pick). * Load index minimum: 106/104 * Speed index minimum: Q * Tubeless * Tread: All Season with M+S approval (and marking on sidewall of tire) * Other: Good performance on snow and ice.   **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **27.** | * Tire dimension: 195/65 R 15 * To be suitable for: Golf 6 - Skoda Octavia. * Load index minimum: 91 * Speed index minimum: H * Tubeless * Tread: All Season with M+S approval (and marking on sidewall of tire) * Other: Good performance on snow and ice.   **Estimated quantity required: 20** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **28.** | • | Tire dimension: 195/65 R 15 |  |  |  |
|  | • | To be suitable for: Golf 6 - Skoda Octavia. |  |  |  |
|  | • | Load index minimum: 91 |  |  |  |
|  | • | Speed index minimum: T |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter with M+S approval (and marking on sidewall of tire) |  |  |  |
|  | * . | **Wet** **grip class not below C (A, B or C) - - according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Good performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 20** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **29.** | • | Tire dimension: 195/60 R 16 |  |  |  |
|  | • | To be suitable for: Toyota Urban Cruiser |  |  |  |
|  |  | 1.4D – 4D AWD |  |  |  |
|  | • | Load index minimum: 89 |  |  |  |
|  | • | Speed index minimum: T |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: All Season with M+S approval |  |  |  |
|  |  | (And marking on sidewall of tire) |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: good performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **30.** | • | Tire dimension: 195/75 R 16C |  |  |  |
|  | • | To be suitable for: (Commercial Light |  |  |  |
|  |  | Trucks) Mercedes Sprinter 518CDI |  |  |  |
|  | • | Load index minimum: 107 / 105 |  |  |  |
|  | • | Speed index minimum: R |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  |  |  |  |  |  |
|  |  | **Wet** **grip class not below C (A, B or C) -** |  |  |  |
|  |  | **- according to EU regulation 1222/2009** |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **31.** | * Tire dimension: 195/75 R 16C * To be suitable for: (Commercial Light Trucks) Mercedes Sprinter 518CDI * Load index minimum: 107 / 105 * Speed index minimum: R * Tubeless * Tread: All Season with M+S approval (and marking on sidewall of tire) * Other: Excellent performance on snow and ice.   **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **32.** | • | Tire dimension: 205/55 R 16 |  |  |  |
|  | • | To be suitable for: VW-Golf VI, |  |  |  |
|  |  | Skoda Superb. |  |  |  |
|  | • | Load index minimum: 91 |  |  |  |
|  | • | Speed index minimum: T |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  |  | **Wet** **grip class not below C (A, B or C) -**  **- according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **33.** | • | Tire dimension: 205/55 R 16 |  |  |  |
|  | • | To be suitable for: VW-Golf VI, |  |  |  |
|  |  | Skoda Superb. |  |  |  |
|  | • | Load index minimum: 91 |  |  |  |
|  | • | Speed index minimum: H |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: All Season, with M+S approval |  |  |  |
|  |  | (and marking on sidewall of tire) |  |  |  |
|  |  |  |  |  |  |
|  |  | Other: Good performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **34.** | • | Tire dimension: 235/55 R 17 |  |  |  |
|  | • | To be suitable for: |  |  |  |
|  |  | BMW / X3 D X drive |  |  |  |
|  | • | Load index minimum: 103 |  |  |  |
|  | • | Speed index minimum: H |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  |  | **Wet** **grip class not below C (A, B or C) -**  **- according to EU regulation 1222/2009** |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  |  |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **35.** | • | Tire dimension: 235/55 R 17 |  |  |  |
|  | • | To be suitable for: |  |  |  |
|  |  | BMW / X3 D X drive |  |  |  |
|  | • | Load index minimum: 103 |  |  |  |
|  | • | Speed index minimum: H |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: All Season, with M+S approval |  |  |  |
|  |  | (And marking on sidewall of tire) |  |  |  |
|  | • Other: Excellent performance on snow and ice. | |  |  |  |
|  |  |  |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **36.** | • | Tire dimension: 205/65 R 16C |  |  |  |
|  | • | To be suitable for: (Commercial Light |  |  |  |
|  |  | Trucks) Mercedes Vito 115C |  |  |  |
|  | • | Load index minimum: 107 / 105 |  |  |  |
|  | • | Speed index minimum: T |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  |  | **Wet** **grip class not below C (A, B or C) -**  **- according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **37.** | * Tire dimension: 205/65 R 16C * To be suitable for: (Commercial Light Trucks) Mercedes Vito 115C * Load index minimum: 107 / 105 * Speed index minimum: T * Tubeless * Tread: All Season, with M+S approval (and marking on sidewall of tire) * Other: Excellent performance on snow and ice.   **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **38.** | * Tire dimension: 205/75 R 16C * To be suitable for: Mercedes Sprinter 515 CDI. * Load index minimum: 113/111 * Speed index minimum: S * Tubeless * Tread: Winter with M+S approval (and marking on sidewall of tire) * **Wet grip class not below C (A, B or C) - according to EU regulation 1222/2009** * Other: Excellent performance on snow and ice.   **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **39.** | * Tire dimension: 215/65 R 16 * To be suitable for: VW Tiguan 2.0TDI * Load index minimum: 98 * Speed index minimum: H * Tubeless * Tread: All Season with M+S approval (and marking on sidewall of tire) * Other: Excellent performance on snow and ice.   **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **40.** | • | Tire dimension: 215/65 R 16 |  |  |  |
|  | • | To be suitable for: VW Tiguan 2.0TDI |  |  |  |
|  | • | Load index minimum: 98 |  |  |  |
|  | • | Speed index minimum: H |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  | * **Wet grip class not below C (A,B or C) - according to EU regulation 1222/2009** | **Wet grip class not below C (A, B or C) - according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **41.** | • | Tire dimension: 215/65 R 16C |  |  |  |
|  | • | To be suitable for: (Commercial Light |  |  |  |
|  |  | Trucks) VW - Transporter T5 2.5TDI 4x4 |  |  |  |
|  |  | Ambulance |  |  |  |
|  | • | Load index minimum: 109 / 107 |  |  |  |
|  | • | Speed index minimum: R |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  | * **Wet grip class not below C (A,B or C) - according to EU regulation 1222/2009** * **Wet grip class not below C (A,B or C) - according to EU regulation 1222/2009** | **Wet grip class not below C (A, B or C) - according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **42.** | • | Tire dimension: 215/65 R 16C |  |  |  |
|  | • | To be suitable for: (Commercial Light |  |  |  |
|  |  | Trucks)VW - Transporter T5 2.5TDI 4x4 |  |  |  |
|  |  | Ambulance |  |  |  |
|  | • | Load index minimum: 109 / 107 |  |  |  |
|  | • | Speed index minimum: R |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: All Season with M+S approval.  marking on sidewall of tire) |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent stability and braking performance on dry and wet surface, suitable for on and off-road conditions. |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **43.** | • | Tire dimension: 225/65 R 16C |  |  |  |
|  | • | To be suitable for: Renault MASTER |  |  |  |
|  |  | Ambulance |  |  |  |
|  |  |  |  |  |  |
|  | • | Load index minimum: 112 / 110 |  |  |  |
|  | • | Speed index minimum: R |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: All Season with M+S approval.  marking on sidewall of tire) |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent stability and braking performance on dry and wet surface, suitable for on and off-road conditions. |  |  |  |
|  |  | **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **44.** | • | Tire dimension: 225/65 R 16C |  |  |  |
|  | • | To be suitable for: Renault MASTER |  |  |  |
|  |  | Ambulance |  |  |  |
|  |  |  |  |  |  |
|  | • | Load index minimum: 112 / 110 |  |  |  |
|  | • | Speed index minimum: R |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  | * **Wet grip class not below C (A,B or C) - according to EU regulation 1222/2009** * **Wet grip class not below C (A,B or C) - according to EU regulation 1222/2009** | **Wet grip class not below C (A, B or C) - according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 2** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **45.** | • | Tire dimension: 215/75 R17.5 |  |  |  |
|  | • | **Must be suitable for**: Mercedes Sprinter with |  |  |  |
|  |  | B6 armoring. |  |  |  |
|  | • | Load index minimum: 126 / 124 |  |  |  |
|  | • | Speed index minimum: M |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: All Season with M+S approval |  |  |  |
|  |  | (And marking on sidewall of tire) to be used on all axles (trailer profile will not be accepted). |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |
|  |  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **46.** | * Tire dimension: 225/55 R 16 * To be suitable for: Audi A6. * Load index minimum: 95 * Speed index minimum: H * Tubeless * Tread: All Season with M+S approval (and marking on sidewall of tire) * Other: Excellent performance on snow and ice.   **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **47.** | • | Tire dimension: 225/75 R 16C |  |  |  |
|  | • | To be suitable for: (Commercial Light |  |  |  |
|  |  | Trucks) Mercedes Sprinter 318CDI 4x4 |  |  |  |
|  | • | Load index minimum: 121 / 120 |  |  |  |
|  | • | Speed index minimum: R |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  | * **Wet grip class not below C (A,B or C) - according to EU regulation 1222/2009** | **Wet grip class not below C (A, B or C) - according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **48.** | • | Tire dimension: 225/75 R 16C |  |  |  |
|  | • | To be suitable for: (Commercial Light |  |  |  |
|  |  | Trucks) Mercedes Sprinter 318CDI 4x4 |  |  |  |
|  | • | Load index minimum: 121 / 120 |  |  |  |
|  | • | Speed index minimum: R |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | * Tread: All Season with M+S approval (and marking on sidewall of tire) * ECE approval (E(#), e(#) * Other: Good performance on snow and ice. |  |  |  |
|  |  | Other: Excellent performance on snow and ice. |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  | **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **49.** | * Tire dimension: 225/65 R 17 * To be suitable for: Toyota RAV4 2.2D-4D * Load index minimum: 102 * Speed index minimum: H * Tubeless * Tread: All Season with M+S approval (and marking on sidewall of tire) * Other: Excellent performance on snow and ice, good off-road performance.   **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **50.** | • | Tire dimension: 225/65 R 17 |  |  |  |
|  | • | To be suitable for: Toyota RAV4 |  |  |  |
|  |  | 2.2D-4D |  |  |  |
|  | • | Load index minimum: 102 |  |  |  |
|  | • | Speed index minimum: H |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  | * **Wet grip class not below C (A,B or C) - according to EU regulation 1222/2009** | **Wet grip class not below C (A, B or C) - according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **51.** | • | Tire dimension: 235/65 R 16C |  |  |  |
|  | • | To be suitable for: (Commercial Light |  |  |  |
|  |  | Trucks) Mercedes Sprinter 318CDI |  |  |  |
|  | • | Load index minimum: 115/113 |  |  |  |
|  | • | Speed index minimum: R |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  | * **Wet grip class not below C (A,B or C) - according to EU regulation 1222/2009** | **Wet grip class not below C (A, B or C) - according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice. |  |  |  |
|  |  | **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **52.** | • | Tire dimension: 235/65 R 16C |  |  |  |
|  | • | To be suitable for: (Commercial Light |  |  |  |
|  |  | Trucks) Mercedes Sprinter 318CDI |  |  |  |
|  | • | Load index minimum: 115/113 |  |  |  |
|  | • | Speed index minimum: R |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: All Season with M+S approval. |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent stability and braking performance on dry and wet surface, suitable for on and off-road conditions. |  |  |  |
|  |  | **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **53.** | * Tire dimension: 235/85 R16 * To be suitable for: Toyota land Cruiser HZJ78L, HZJ105L (B4 armored) * Load index minimum: 120 /116 * Speed index minimum: Q * Tubeless * Tread: All Season with M+S approval (and marking on sidewall of tire) * Other: Excellent performance on snow and ice and good off-road performance.   **Estimated quantity required: 4** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **54.** | * Tire dimension: 235/65 R17 * To be suitable for: VW Touareg GP 2.5TDI R5 * Load index minimum: 108 * Speed index minimum: H * Tubeless * Tread: All Season with M+S approval (and marking on sidewall of tire) * Other: Excellent performance on snow and ice and good off-road performance.   **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **55.** | • | Tire dimension: 235/70 R16 |  |  |  |
|  | • | To be suitable for: Nissan Pathfinder |  |  |  |
|  |  | (R51M) |  |  |  |
|  | • | Load index minimum: 106 |  |  |  |
|  | • | Speed index minimum: T |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: All Season with M+S approval (and marking on sidewall of tire) |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow and ice and good off-road performance. |  |  |  |
|  |  | **Estimated quantity required:40** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **56.** | • | Tire dimension: 235/70 R16 |  |  |  |
|  | • | To be suitable for: Nissan Pathfinder |  |  |  |
|  |  | (R51M) |  |  |  |
|  | • | Load index minimum: 106 |  |  |  |
|  | • | Speed index minimum: T |  |  |  |
|  | • | Tubeless |  |  |  |
|  | • | Tread: Winter, M+S approval (and marking on sidewall of tire) |  |  |  |
|  | * **Wet grip class not below C (A,B or C) - according to EU regulation 1222/2009** | **Wet grip class not below C (A, B or C) - according to EU regulation 1222/2009** |  |  |  |
|  |  |  |  |  |  |
|  | • | Other: Excellent performance on snow, ice and off-road.  “ |  |  |  |
|  |  | **A tire with a tread pattern and structure designed to better performance in snow than that of a normal tire marked with, so called, Alpine symbol.**  **Estimated quantity required: 100** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **57.** | * **Tire dimension: 275/70R18** * To be suitable for: Toyota Land Cruiser – VDJ200L (B6 armored by STOOF) * Load index minimum: 128 / 125 * Speed index minimum: Q * Tubeless * Tread: H/T / with M+S approval (and marking on sidewall of tire). * Other: Excellent performance on snow and ice.   **Estimated quantity required : 100** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **58.** | * Tire dimension: 285/60R18 * To be suitable for: Toyota Land Cruiser – VDJ200L (B6 armored by STOOF) * Load index minimum: 120 * Speed index minimum: R * Tubeless * Tread: All Season / All Terrain with M+S approval (and marking on sidewall of tire) * Other: Excellent performance on snow and ice.   **Estimated quantity required: 10** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **INNER TUBES** | | | | |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** | | | | | |
| **59.** | * Tube dimensions to be suitable for tire size: 12.00 R 20 * To be used for: Truck -Volvo NL10 (split rim)   **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **60.** | * Tube dimension to be suitable for tire size: 12.00 R 18 * To be used for: Torpedo T1 - Armored Personnel Carrier (split rim)   **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **61.** | * Tube dimensions to be suitable for tire   size: 8.25 R 16   * To be used for: Hyundai HD120 Truck (split rim)   **Estimated quantity required: 8** |  |  |  |
| **62.** | * Tube dimensions to be suitable for tire   size: 8.25 (8.15) – 15   * To be used for: Forklifts Daewoo D70S-2, Daewoo D30S-3 (front)   **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **63.** | * Tube dimension to be suitable for tire size: 6.50– 10 * To be used for: Forklift Daewoo D30S-3 (rear)   **Estimated quantity required: 8** |  |  |  |
| **Tire Flaps** (for use with split rims) | | | | |
| **64.** | * Flap dimension to be suitable for tire size: 12.00 R 20 * To be used for: Truck -Volvo NL10 (split rim)     **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **65.** | * Flap dimension to be suitable for tire size: 12.00 R 18 * To be used for: Torpedo T1 - Armored Personnel Carrier (split rim)   **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **66.** | * Flap dimension to be suitable for tire size: 8.25 R 16 * To be used for: Hyundai HD120 Truck (split rim)   **Estimated quantity required: 8** |  |  |  |
| **67.** | * Flap dimension to be suitable for tire size: 8.25 (8.15) – 15 * To be used for: Forklifts Daewoo D70S-2, Daewoo D30S-3 (front)   **Estimated quantity required: 8** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **68.** | * Flap dimension to be suitable for tire size: 6.50– 10 * To be used for: Forklift Daewoo D30S-3 (rear)   **Estimated quantity required: 8** |  |  |  |
| **Tubeless Valves** | | | | |
| **69.** | * TR 413   **Estimated quantity required: 200** |  |  |  |
| **70.** | * TR 414   **Estimated quantity required: 200** |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **71.** | * TR 415   **Estimated quantity required: 200** |  |  |  |
| **72.** | * TR 416   **Estimated quantity required: 60** |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **.**  **Item Number** |  | **2.**  **Specifications Required** | **3.**  **Specifications Offered (incl. brand/model)** | **4.**  **Notes, remarks, ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| **73.** | * TR 621 A   **Estimated quantity required: 40** | |  |  |  |